   _____________________________________________________________________  
 ,/                                                                     \,
 |     .,-:::::/   :::.      ...    :::  .,-:::::   ::   .: .,::::::     |
 |   ,;;-'````'    ;;`;;     ;;     ;;;,;;;'````'  ,;;   ;;,;;;;''''     |
 |   [[[   [[[[[[/,[[ '[[,  [['     [[[[[[        ,[[[,,,[[[ [[cccc      |
 |   "$$c.    "$$c$$$cc$$$c $$      $$$$$$        "$$$"""$$$ $$""""      |
 |    `Y8bo,,,o88o888   888,88    .d888`88bo,__,o, 888   "88o888oo,__    |
 |      `'YMUP"YMMYMM   ""`  "YmmMMMM""  "YUMMMMMP"MMM    YMM""""YUMMM   |
 |                                                                       |
 |           ~ E ~ L ~ E ~ C ~ T ~ R ~ O ~ S ~ O ~ U ~ N ~ D ~           |
 '\_____________________________________________________________________/'
 ,/                                                                     \,
 |   G500 FORMAT JUMBLER                                                 |
 |                                                                       |
 |     Connects signals from one kind of  cable like a 1/4" jack, to     |
 |     another, either 3.5mm (minijack), or 4mm banana jack.             |
 |                                                                       |
 |     A 0V ground reference is included to share common ground with     |
 |     banana systems.                                                   |
 |                                                                       |
 |     The module is separated into pairs of rows. The top row has a     |
 |     white banana jack, the bottom has a red banana jack.              |
 |                                                                       |
 |     This module also  features stereo splitting/joining. Plugging     |
 |     a TRS cable into either the  minijack or 1/4" jack of a white     |
 |     row will connect the "ring" of  the cable to the "tip" of the     |
 |     other format. To  put another way, two 1/4"  jack signals can     |
 |     be sent over a single minijack TRS cable, or vice versa. This     |
 |     can  be used  to bundle  signals together  before going  to a     |
 |     mixer that uses TRS inputs,  or splitting a insert jack (e.g.     |
 |     on a mixer or compressor), and  sending the signal over to be     |
 |     processed in modular before sending back on the same cable.       |
 |                                                                       |
 |   ~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~   |
 |                                                                       |
 |       > Price ....... 120 USD                                         |
 |       > Release ..... October 31 2025                                 |
 |       > Format ...... 5U (DOTCOM power)                               |
 |       > Depth ....... ~35mm                                           |
 |       > Power ....... +15V @ 0mA                                      |
 |                       -15V @ 0mA                                      |
 |                       +5V  @ 0 A                                      |
 |       > Controls .... None                                            |
 |       > Inputs ...... White rows:     4mm Banana,                     |
 |                                       TRS Minijack                    |
 |                                       TRS 1/4" jack                   |
 |                       Red Rows:       4mm Banana,                     |
 |                                       TS Minijack                     |
 |                                       TRS 1/4" jack                   |
 |                       Black banana:   Direct connection to ground*    |
 |                       ~0R input impedance**                           |
 |                       +/-15V accepted***                              |
 |       > Outputs ..... Interchangable with inputs                      |
 |       > Notes ....... * Ground references usually connect to PSUs     |
 |                       ** all wiring and copper has some impedance     |
 |                       *** caution should   be   excercised   when     |
 |                          from +/-15V going  systems to  +/-12V or     |
 |                          lower voltagother  e setups,  as it  may     |
 |                          clipping or introduce  damage  a  module     |
 |                          no overvoltadesigned with ge protection.     |
 |                          Please patchresponsibly.                     |
 '\_____________________________________________________________________/'
par:74jp7s6
vim:ve=all:expandtab
