   _____________________________________________________________________ 
 ,/                                                                     \,
 |     .,-:::::/   :::.      ...    :::  .,-:::::   ::   .: .,::::::     |
 |   ,;;-'````'    ;;`;;     ;;     ;;;,;;;'````'  ,;;   ;;,;;;;''''     |
 |   [[[   [[[[[[/,[[ '[[,  [['     [[[[[[        ,[[[,,,[[[ [[cccc      |
 |   "$$c.    "$$c$$$cc$$$c $$      $$$$$$        "$$$"""$$$ $$""""      |
 |    `Y8bo,,,o88o888   888,88    .d888`88bo,__,o, 888   "88o888oo,__    |
 |      `'YMUP"YMMYMM   ""`  "YmmMMMM""  "YUMMMMMP"MMM    YMM""""YUMMM   |
 |                                                                       |
 |           ~ E ~ L ~ E ~ C ~ T ~ R ~ O ~ S ~ O ~ U ~ N ~ D ~           |
 '\_____________________________________________________________________/'
 ,/                                                                     \,
 |   G315 STATIC WAVEFOLDER                                              |
 |                                                                       |
 |     Classic  serial  wavefolder  topology, with  additional  gain     |
 |     between each stage.  The added gain multiplies  the number of     |
 |     folds from the previous stage;  the total number of folds for     |
 |     each stage  is then (3^n)-1, or  2, 8, and 26  folds for each     |
 |     stage, respectively.                                              |
 |                                                                       |
 |     Additionally, this topology creates formant like behaviors at     |
 |     the 3rd stage output. As each stage has gain added, the slope     |
 |     of the resulting  wave will not only fold  over, but increase     |
 |     in  degree as  the input  voltage approaches  0. Formant-like     |
 |     tones  come out  as a  result,  though these  will always  be     |
 |     harmonically locked to the  input frequency. In practice, for     |
 |     example, it can  make a sawtooth wave sound a  lot like a car     |
 |     engine.                                                           |
 |                                                                       |
 |     This module  was designed  for applying nonlinear  control to     |
 |     CV  inputs,  as  well  as an  extreme  distortion  unit.  The     |
 |     folding behavior creates differently  spaced deadzones in the     |
 |     voltage transfer function, resulting  in a gated-fuzz at some     |
 |     settings, and high-gain distortion at others.                     |
 |                                                                       |
 |   ~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~*~   |
 |                                                                       |
 |       > Price ....... 140 USD                                         |
 |       > Release ..... November 21 2025                                |
 |       > Format ...... Eurorack                                        |
 |       > Depth ....... ~20mm                                           |
 |       > Power ....... +12V @ 10mA                                     |
 |                       -12V @ 10mA                                     |
 |                       +5V  @ 0 A                                      |
 |       > Controls .... Offset    - Apply DC offset                     |
 |                       Folds     - Input attenuator                    |
 |                       Feedback  - Attenuator, aux input               |
 |       > Inputs ...... In        - Attenuated with "Folds" knob        |
 |                       Unity     - Unattenuated input                  |
 |                       In-FDBK   - Replaces 3rd stage feedback         |
 |                       100K input impedance                            |
 |                       +/- 5V nominal, +/-12V accepted                 |
 |       > Outputs ..... 1         - First stage output                  |
 |                       2         - Second stage output, inverted       |
 |                       3         - Third stage output                  |
 |                       1K output impedance                             |
 |                       +/-5V nominal, +/-12V likely                    |
 |       > Notes ....... Same circuit as G515 in 5U                      |
 '\_____________________________________________________________________/'
 par:75jp7s7
 vim:ve=all:expandtab 
